set port /dev/tty.usbmodem4031
set baudrate 250000
set monitor True
set last_bed_temperature 60.0
set last_temperature 150.0
set extruders 1
set build_dimensions 190.00x195.00x100.00-5.00+0.00+0.00+200.00+0.00+0.00
set light3d False
set lockonstart True
set xy_feedrate 2750
set z_feedrate 100
set e_feedrate 50
set last_extrusion 3
set last_file_path /Users/jannik/Desktop
button 0 "getEndstop" M119
button 1 "getPosition" M114
button 2 "Fan on" M106 S255
button 3 "Fan off" M107
button 4 "goStartPos" G1 F3000 X50 Y100 Z5
button 5 "goMiddle" G1 F3000 X100 Y100
button 6 "set Z0" G92 Z0
button 7 "set Z20" G92 Z20
button 9 "setPP" G92 X100 Y100 Z20
set slicecommand /Applications/Development/Slic3r.app/Contents/MacOS/slic3r $s --output $o
set sliceoptscommand /Applications/Development/Slic3r.app/Contents/MacOS/slic3r
set uimode Compact
set slic3rintegration True
set mainviz 2D
set preview_extrusion_width 0.4
set bedtemp_pla 60
set temperature_pla 190
set last_window_maximized False
set last_window_width 1060
set last_window_height 530
set last_sash_position 400
set tempgauges True
set lockbox True
set recentfiles ["/Users/jannik/Desktop/endstop_clip-X-#79779--h0.3f30%.gcode", "/Users/jannik/Desktop/endstop-clamp--h0.3f30%.gcode", "/Users/jannik/Desktop/i3-z-endstop--h0.3f30%.gcode", "/Users/jannik/Desktop/endstop-X-#818317--h0.3f30%.gcode", "/Users/jannik/Desktop/RaspberryPiStand--h0.3f30%.gcode"]
set total_filament_used 11841.2725058
button 8 "goParkPos" /c "green" G1 F3000 X100 Y100 Z20
set clamp_jogging True
button 10 "goAccessPos" G1 F3000 X180 Y190
macro goAway
  G91     ; relative positioning
  G0 Z5  ; rise Z axis
  G90     ; turn absolute positioning back on
  G1 F3000 X180
button 11 "goAway" /c "red" goAway
set controlsmode Standard
set viz3d False
